SECTION 09852

2-DIMENSIONAL SOUND DIFFUSER (Omniffusor® U84)


PART 1 GENERAL

1.01 SECTION INCLUDES

A. 2-Dimensional Sound Diffuser: Quadratic Residue Diffuser, Model Omniffusor® U84
B. Coordination with all trades having elements that attach to, penetrate through or are concealed behind/above the panels of this section. 

1.02 PRODUCTS INSTALLED BUT NOT SUPPLIED UNDER THIS SECTION

A. Wood mounting battens if required. 

1.03 RELATED SECTIONS

A. Section 06420 – Wood Paneling
B. Section 09120 – Suspension Framing/Furring for Plaster/Gypsum Board Assemblies
C. Section 09250 – Gypsum Board
D. Division 15 Sections – Mechanical Work
E. Division 16 Sections – Electrical Work
F. Division 17 Sections – Audio, Data, Telecommunication Work

1.04 DEFINITIONS

A. 2-Dimensional Sound Diffusers can be either installed as independent units or in an array to form a larger unit.

1.05 ALTERNATES

A. Prior Approval: Proposed substitutions for products in this section may be submitted to the architect and acoustical consultant no later than ten (10) working days prior to the bid due date.  Substitutions shall only be considered if submitted with complete information including acoustic data and a sample not smaller than 59 cm x 59 cm (23” x 23”) showing product design, composition and finish.  Acceptance of substituted products is contingent on the architect’s and acoustical consultant’s approval and the substitution’s compliance with all specified criteria.  The architect shall approve substitution request via addendum.
B. Unapproved Substitutions.  Substitutions not approved via addendum shall not be submitted to the architect or acoustical consultant.

1.06 REFERENCES

A. Local Building Code – Current Edition
B. International Organization for Standardization
1. ISO 354 Measurement of Sound Absorption in a Reverberation Room
2. ISO 10534 - Determination of sound absorption coefficient and impedance in impedance tubes - Part 1: Method using standing wave ratio.
3. ISO 17497-1 Sound-scattering properties of surfaces- Part 1: Measurement of the random-incidence scattering coefficient in a reverberation room.
C. AES-4id-2001: AES Information Document for Room Acoustics & Sound Reinforcement Systems – Characterization & Measurement of Surface Scattering Uniformity.
D. American Society for Testing & Materials (ASTM)
1. ASTM E 1050-98 - Standard Test Method for Impedance and Absorption of Acoustical Materials Using a Tube, Two Microphones, and a Digital Frequency Analysis System
2. ASTM C 423 - Sound Absorption & Sound Absorption Coefficients by the Reverberation Room Method
3. ASTM E 84: Standard Test Method for Surface Burning Characteristics of Building Materials
E. Published technical papers
1. T.J. Cox, B-I.Dalenback, P. D’Antonio, J.J. Embrechts, J.Y. Jeon, E. Mommertz and M. Vorlaender, “A tutorial on scattering and diffusion coefficients for room acoustic surfaces”, Acta Acustica uW Acustica, 92, 1-15 (2006)
2. AES-4id-2001, “AES Information document for room acoustics and sound  reinforcement systems- Characterization and measurement of surface scattering uniformity”, J. Audio Engineering Soc., 49(3), 149-165 (2001)
3. E. Mommertz, Appl. Acoust., 60(2), 201-204 (2000)
		
1.07 SYSTEM DESCRIPTION

A. Design Requirements: 2-Dimensional Sound Diffusers shall be based on the 2-dimensional reflection phase grating principal, using an array of square wells separated by thin dividers.  The depth of the wells shall be based on the phase shifted prime 7 quadratic residue number theory sequence. 

B. Performance Requirements:

1. Random Incidence Sound Absorption Coefficients (a): Tested by independent, accredited, NVLAP facility according to ASTM C 423 and ASTM E 795 for an E mounting.

	125 Hz	250 Hz	500 Hz	1000 Hz	2000 Hz	4000 Hz

	0.12	0.10	0.14	0.22	0.06	0.12

2. Noise Reduction Coefficient (NRC): Tested by independent, accredited, NVLAP facility according to ASTM C 423 and ASTM E 795 for an E mounting.

Noise Reduction Coefficient = 0.14

3. Third-octave band acoustical performance requirements from 100 Hz to 4000 Hz for random incidence sound absorption shall be measured according to ASTM C423 or ISO 354; the normalized random incidence diffusion coefficient shall be the average of measured or calculated directional diffusion coefficients, according to AES-4id-2001 at -60, -30, 0, 30, and 60 degrees and the random incidence scattering coefficient shall be measured according to ISO- 17497-1 (Scattering (ISO)) or determined from the average of the measured directional correlation scattering coefficients (Scattering (c)) according to the method of Mommertz [Reference 1.05/E1 and 1.05/E3].  Directional polar responses, which indicate the uniformity of scattering in third-octave bands, for sample and reference reflector, shall be provided to the acoustical consultant for approval. The random incidence coefficients shall be what are indicated in the table below:

	

	f (Hz)
	Diffusion

	400
	0.01

	500
	0.02

	630
	0.02

	800
	0.08

	1000
	0.41

	1250
	0.30

	1600
	0.49

	2000
	0.43

	2500
	0.43

	3150
	0.67

	4000
	0.54



1.08 SUBMITTALS

A. Product Data: Submit manufacturers’ technical data including basic system description, options and component sizes.  Identify all applicable features and options.  Cross out any inapplicable features or options.
B. Shop Drawings: The contractor shall produce and submit shop drawings of products and suspension or mounting systems overlaid on base drawings (interior elevations or reflected ceiling plans) supplied electronically by the architect.  Show overall layout with dimensions and references to details as necessary for penetrations, joints, ends and intersections with other materials or building components.  Submit schedule of all quantities, sizes, hole patterns, edge banding, borders, veneers and finishes.  Field-verify site conditions with dimensions shown on shop drawings.
C. Samples: Minimum 29.2 cm (11-1/2”) x 22.9 cm (9”) sample of specified panel and color.
D. Certifications: Manufacturers’ certifications that products comply with specified requirements, including laboratory reports showing compliance with specified tests and standards.

1.09 QUALITY ASSURANCE

A. Qualifications: Manufacturer and installation contractor shall have a minimum of three years of experience with similar systems.
B. Single Source: All products under this section shall be supplied by a single manufacturer to ensure consistency in product size and finish.

C. Flame Spread / Smoke Developed Characteristics: Product components tested by independent, accredited NVLAP facility according to ASTM E 84 and NFPA 255. 
1. Composite Flame Spread Rating: 25 (maximum)
2. Smoke Developed: 450 (maximum)
D. Pre-Installation Meeting: Installing contractor shall organize and conduct pre-installation meetings with all other trades to coordinate substrate conditions, conditioning of the space (temperature & humidity), and elements attaching to, penetrating through or concealed above/behind work in this section.

1.010 DELIVERY STORAGE AND HANDLING

A. Shipping, Handling and Unloading: Deliver panels to the project site in the manufacturer’s original, unopened packaging.  Do not unpack or handle finished products until the project environmental requirements have been met and the products are ready to be installed.
B. Storage and Protection: Protect products from damage that may be caused by exposure to water, chemicals, direct sunlight or infestation.   
C. Acceptance at Site: Ensure that all project environmental requirements have been met prior to unpacking or installing wood panels and all associated wood trim products.  Full or partial installation constitutes complete product acceptance.
D. Waste Management and Disposal: Dispose of all packaging materials and debris in a safe and environmentally responsible manner according to the instructions set forth by the General Contractor, local ordinances or codes and the Environmental Protection Agency. 

1.011 PROJECT CONDITIONS

A. Project Environmental Requirements: Installation area shall be enclosed, protected from weather and be temperature and humidity controlled prior to unpacking and installing Diffusers.
 
B. [bookmark: _Hlk163220801]Product Handling: Handle panels carefully so as to avoid chipping, scratching, scuffing or denting.
.

1.012 WARRANTY

A. Submit to Owner or Owner’s Representative a written and dated warranty issued by the ceiling/wall manufacturer warranting the panels and associated trim pieces against defects in materials or manufacturing for a period of one (1) year from the date of delivery.
B. Components used in the system but not provided by the manufacturer are excluded from the manufacturer’s warranty.  Damage caused by exposure to moisture or rapid or extreme changes to temperature or humidity are excluded from the manufacturer’s warranty.  Damage caused by improper storage, handling, acclimatization, or installation is excluded from the warranty.  Appearances and colorings can vary over time and as site conditions change and are therefore excluded from the warranty.

1.013 OWNER’S INSTRUCTIONS

A.	Installing contractor shall provide to the building owner or to the owner’s representative a copy of the manufacturer’s maintenance manual supplied with the panels. 

1.014 MAINTENANCE

A. Extra Materials: If provided per the project requirements, extra materials shall remain in the manufacturer’s original, unopened packaging and shall be given to the building owner or owner’s representative upon substantial completion of work.

PART 2 PRODUCTS

2.01 MANUFACTURER

A.	RPG Acoustical Systems, LLC, 99 South St, Passaic, NJ 07055 (telephone) (973-916-1166, http://www.rpgacoustic.com.

2.02 MATERIALS

A. [bookmark: _Hlk163220853]Polymer (1/4”) 

B. Color: Black or White


2.03 MANUFACTURED UNITS

A. Unit Dimensions
1. Standard 2 x 2 Units: Height 23-5/8”, Width 23-5/8”, Depth 4”

B. Weight
1. Standard 2 x 2 Units: 15 pounds (maximum)

2.04 ACCESSORIES

A.	Units are supplied with (4) deepest center wells uncovered.  Use exposed well blocking to attach through to substrate, then cover with supplied (4) well covers.


PART 3 EXECUTION

3.01 INSTALLERS

A.	Installing contractor shall have a minimum of five (5) years successful experience installing ceiling and wall systems in similar applications using similar mounting techniques or suspension systems.

3.02 EXAMINATION

A. Site Verification of Conditions: Examine installation area for compliance with all manufacturers’ project environmental requirements and ensure uninstalled products have been stored, handled and acclimatized properly prior to commencing installation.  Inspect all substrates for completion and quality of work to ensure that surfaces are level, plumb, clean, dry and completely cured from water or solvent evaporation.  Do not commence installation if the structural capacity of the substrate is questionable or inadequate.
B. Coordination with Other Trades: Coordinate with all other trades to ensure that wet work including concrete, terrazzo, plastering, painting, etc. in the installation area is complete, cured and dry prior to installation.  Coordinate with all other trades to verify that components associated with mechanical, electrical, lighting, data, telecommunication, audio, video, fire suppression and other building systems are installed behind or above designated installation areas prior to commencing installation.  Coordinate the exact size, location and sequencing of building system components that penetrate the ceiling/wall panels.

3.03 PREPARATION

A. Protection: Protect all floor, wall and ceiling finishes against possible damage prior to commencing installation and during installation.
B. Surface Preparation: When necessary, field measure substrates to acquire accurate dimensions of panels and submit final dimensions to manufacturer.
C. Dry Fit (Joining Units Only): Prior to commencing installation of joining units, unpack all diffuser pieces and set pieces on clean, soft, dry surface.  Ensure that all pieces are present and dry fit all pieces together.
D. Field Measure: Prior to commencing installation, measure diffusers (standard units or dry-fit joining units) and ensure that dimensions correspond to field measured dimensions of installation area.   

3.04 INSTALLATION

A. Install panels as shown and detailed in the architectural drawings and according to manufacture’s guidelines and industry standards.
B. Install panels with a minimum ¼” gap between any adjacent units both vertically and horizontally. 
C. Install diffusers by fastening through (4) deepest center wells to substrate.  Cover with supplied (4) well covers. 
D. Install units so that finished side with wells faces into occupied space.

3.05 CONSTRUCTION

A. Interface with Other Work: Support all light fixtures, HVAC air inlet/outlet devices, speakers, signage, sprinkler heads/piping, etc. independently from wood panels.  Contractor shall not use panels to support the weight of any other building element or component. 

3.06 ADJUSTING

A. Following initial installation, adjust mounting hardware or suspension system so that removable panels can be removed easily, yet stay safely secured upon replacement.  Adjust panels so that surfaces are aligned, flush and level or plumb and gaps in between units are of a consistent width and straight. 
B. Check that manufacturer’s joining requirements were maintained during installation.  
C. Remove and replace at no extra charge any damaged panels that cannot be repaired to the Owner’s and Architect’s satisfaction.

3.07 CLEANING

A. Remove dust from surfaces and penetrations by vacuuming using only a soft brush.  Do not scratch surfaces with sharp metal or plastic vacuum cleaner extensions.  Remove pencil marks with soft erasure.  Remove general surface dirt with a clean, soft cloth dampened with a diluted, mild, cleaning agent and warm water.  Wipe again with clean, soft cloth dampened only with warm water.  Finally, dry surface completely with clean, dry cloth.  Do not use abrasive cleaners with grit or cloths that could scratch the panel.
B. Remove and replace at no additional charge any materials that cannot be cleaned to the Owner’s satisfaction.

3.08 DEMONSTRATION

A. Demonstrate to the building owner or to the owner’s representative the safe and proper method for removing and replacing all types of accessible panels.
B. Supply the building owner or the owner’s representative with any special tools provided by the manufacturer required to unlatch safety hardware on accessible panels. 

3.09 PROTECTION

A.	Upon completion of work, protect installed panels from damage or soiling until project substantial completion and owner occupancy. 


END OF SECTION
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